PTS test results for GATT

PTS version: 6.1
Tested: 24-April-2015
Android version: 5.1

Results:
PASS	test passed
FAIL	test failed
INC	test is inconclusive
N/A	test is disabled due to PICS setup

-------------------------------------------------------------------------------
Test Name		Result	Notes
-------------------------------------------------------------------------------
TC_GAC_CL_BV_01_C	PASS	haltest:
				gattc scan
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc_uuid>
				gattc write_characteristic: type 3
TC_GAC_SR_BV_01_C	PASS	PTS issue #13073
				TSE #6271
				haltest:
				gatts add_service
				gatts add_chaaracteristic:
					<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
					<data> value greater than MTU
					repeat with correct offset
				gatts send_response:
					<data> value greater than MTU
					repeat with correct offset
TC_GAD_CL_BV_01_C	PASS	haltest:
				NOTE: Repeat following steps if asked
				gattc connect <client_id> <PTS addr>
				gattc search_service <conn_id>
				gattc disconnect <client_if> <PTS bdaddr>
					<conn_id>
TC_GAD_CL_BV_02_C	PASS	haltest:
				NOTE: Repeat following steps if asked
				gattc connect <client_id> <PTS addr>
				gattc search_service <conn_id> <uuid>
				gattc disconnect <client_if> <PTS bdaddr>
					<conn_id>
TC_GAD_CL_BV_03_C	PASS	haltest:
				NOTE: Repeat following steps if asked
				gattc connect <client_id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x2802 0x08
					0x0001 0xffff
				NOTE: Keep on mind MTU size
					(some att rsp could not fit)
				gattc_disconnect <client_if> <PTS bdaddr>
					<conn_id>
TC_GAD_CL_BV_04_C	PASS	haltest:
				NOTE: Repeat following steps if asked
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
TC_GAD_CL_BV_05_C	PASS	haltest:
				NOTE: Repeat following steps if asked
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x2803 0x08
					<start hdl> <end hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAD_CL_BV_06_C	PASS	haltest:
				NOTE: Repeat following steps if asked
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <conn_id> <svc_id>
					<char_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAD_CL_BV_07_C	PASS	haltest:
				NOTE: Repeat following step if asked
				bluetooth get_remote_services
TC_GAD_CL_BV_08_C	PASS	haltest:
				NOTE: Repear following step if asked
				bluetooth get_remote_services
TC_GAD_SR_BV_01_C	PASS	haltest:
				gattc register_client
				gattc listen
TC_GAD_SR_BV_02_C	PASS	haltest:
				gattc register_client
				gattc listen
TC_GAD_SR_BV_03_C	PASS	haltest:
				gattc register_client
				gattc listen
				gatts register_server
				gatts add_service
				gatts start_service
				gatts add_service
				gatts add_included_service
				gatts start_service
TC_GAD_SR_BV_04_C	PASS	haltest:
				gattc register_client
				gattc listen
TC_GAD_SR_BV_05_C	PASS	haltest:
				gattc register_client
				gattc listen
TC_GAD_SR_BV_06_C	PASS	haltest:
				gattc register_client
				gattc listen
TC_GAD_SR_BV_07_C	PASS	haltest:
				when requested:
				bluetooth get_remote_services
				NOTE: check if found requested service
TC_GAD_SR_BV_08_C	PASS	haltest:
				when requested:
				bluetooth get_remote_services
				NOTE: check if found requested service
TC_GAR_CL_BV_01_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <client_id> <svc_id>
					<char_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_01_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x0000
					0x0a <invalid char hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_02_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <client_id> <svc_id>
					<char_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_03_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x0000
					0x0a <inf. auth. att hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_04_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x0000
					0x0a <inf. auth. att hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_05_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <client_id> <svc_id>
					<char_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BV_03_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 0x0001 0xffff
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_06_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_07_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_09_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_10_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_11_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BV_04_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				NOTE: Repeat following steps if asked
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <client_id> <svc_id>
					<char_id>
				NOTE: After reading all characteristics
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_12_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <client_id> <svc_id>
					<char_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_13_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x0000
					0x0c <handle> <offset>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_14_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x0000
					0x0a <char_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_15_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <client_id> <svc_id>
					<char_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_16_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <client_id> <svc_id>
					<char_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_17_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <client_id> <svc_id>
					<char_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BV_05_C	N/A
TC_GAR_CL_BI_18_C	N/A
TC_GAR_CL_BI_19_C	N/A
TC_GAR_CL_BI_20_C	N/A
TC_GAR_CL_BI_21_C	N/A
TC_GAR_CL_BI_22_C	N/A
TC_GAR_CL_BV_06_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_23_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_24_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x0000
					0x0a <desc_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_25_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_26_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_27_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BV_07_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				NOTE: Repeat following step if asked
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				NOTE: After reading all characteristics
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_28_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_29_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x0000
					0x0c <handle> <offset>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_30_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> 0x0000
					0x0a <desc_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_31_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_32_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_33_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc read_descriptor <client_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_CL_BI_34_C	PASS	haltest:
				gattc connect
				gattc test_command 224 <addr> 0 0x0a <handle>
				gattc disconnect
TC_GAR_CL_BI_35_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <client_id> <svc_id>
					<char_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAR_SR_BV_01_C	PASS
TC_GAR_SR_BI_01_C	PASS
TC_GAR_SR_BI_02_C	PASS
TC_GAR_SR_BI_03_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						 <properties> 2 <permissions> 1
				gatts start_service
				gatts send_response: <status> 8
TC_GAR_SR_BI_04_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 3
				gatts start_service
				gatts send_response
TC_GAR_SR_BI_05_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						 <properties> 2 <permissions> 1
				gatts start_service
				gatts send_response: <status> 12
TC_GAR_SR_BV_03_C	PASS
TC_GAR_SR_BI_06_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 16
				gatts start_service
TC_GAR_SR_BI_07_C	PASS
TC_GAR_SR_BI_08_C	PASS
TC_GAR_SR_BI_09_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts start_service
				gatts send_response: <status> 8
TC_GAR_SR_BI_10_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts start_service
				gatts send_response: <status> 5
TC_GAR_SR_BI_11_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts start_service
				gatts send_response: <status> 12
TC_GAR_SR_BV_04_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
TC_GAR_SR_BI_12_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 8 <permissions> 16
				gatts start_service
				gatts send_response
TC_GAR_SR_BI_13_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response: <status> 7
TC_GAR_SR_BI_14_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						 <properties> 2 <permissions> 1
				gatts start_service
				gatts send_response: <status> 1
TC_GAR_SR_BI_15_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						 <properties> 2 <permissions> 1
				gatts start_service
				gatts send_response: <status> 8
TC_GAR_SR_BI_16_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						 <properties> 2 <permissions> 1
				gatts start_service
				gatts send_response: <status> 5
TC_GAR_SR_BI_17_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						 <properties> 2 <permissions> 1
				gatts start_service
				gatts send_response: <status> 12
TC_GAR_SR_BV_05_C	N/A
TC_GAR_SR_BI_18_C	N/A
TC_GAR_SR_BI_19_C	N/A
TC_GAR_SR_BI_20_C	N/A
TC_GAR_SR_BI_21_C	N/A
TC_GAR_SR_BI_22_C	N/A
TC_GAR_SR_BV_06_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor
				gatts start_service
				gatts send_response
TC_GAR_SR_BI_23_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 16
				gatts start_service
TC_GAR_SR_BI_24_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor
				gatts start_service
				gatts send_response: <status> 1
TC_GAR_SR_BI_25_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response: <status> 8
TC_GAR_SR_BI_26_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response: <status> 5
TC_GAR_SR_BI_27_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response: <status> 12
TC_GAR_SR_BV_07_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
TC_GAR_SR_BV_08_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
TC_GAR_SR_BI_28_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 16
				gatts start_service
TC_GAR_SR_BI_29_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response: <status> 7
TC_GAR_SR_BI_30_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response: <status> 1
TC_GAR_SR_BI_31_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response: <status> 8
TC_GAR_SR_BI_32_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response: <status> 5
TC_GAR_SR_BI_33_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permissions> 1
				gatts start_service
				gatts send_response: <status> 12
TC_GAR_SR_BI_34_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic
				gatts start_service
				gatts send_response <status> 0x80-0x9F
TC_GAR_SR_BI_35_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic
				gatts start_service
				gatts send_response <status> 0x80-0x9F
TC_GAW_CL_BV_01_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 1 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BV_02_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 4 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BV_03_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 2 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_02_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x12
					<char_hdl> <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_03_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 2 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_04_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 2 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_05_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 2 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_06_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 2 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BV_05_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc execute_write <conn_id> 1
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_07_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x12
					<char_hdl> <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_08_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc execute_write <conn_id> 1
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_09_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x16
					<char_hdl> <offset> <data>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x18 1
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_11_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_12_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_13_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BV_06_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc execute_write <conn_id> 1
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_14_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x16
					<char_hdl> <offset> <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_15_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_17_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_18_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_19_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 3 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BV_08_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 2 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_20_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x12
					<char_hdl> <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_21_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 2 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_22_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 2 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_23_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 2 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_24_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 2 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BV_09_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 3 <data>
				gattc execute_write <conn_id> 1
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_25_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x16
					<char_hdl> <offset> <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_26_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 3 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_27_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x16
					<char_hdl> <offset> <data>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x18 1
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_29_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 3 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_30_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 3 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_31_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x16
					<desc_hdl> 0x0000 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_32_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x16
					<desc_hdl> <offset> <data>
				gattc test_command 0xe1 <PTS addr> 0x0000 0x18 0
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_33_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 2 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_34_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 2 <value>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_35_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 2 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_CL_BI_36_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 2 <data>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAW_SR_BV_01_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 4 <permissions> 17
				gatts start_service
TC_GAW_SR_BV_02_C	PASS	haltest:
				gatts add service
				gatts add_characteristics:
					<properties> 66 <permisions> 145
				gatts start_service
				gattc listen
				gatts send_response: (twice)
				NOTE: gatts_request_write_cb shall be called
								 (verify it)
TC_GAW_SR_BI_01_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 68
						<permissions> 129
				gatts start_service
				gatts send_response: repeat with <data> 1
TC_GAW_SR_BV_03_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
TC_GAW_SR_BI_02_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response: <status> 1
TC_GAW_SR_BI_03_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 1
				gatts start_service
TC_GAW_SR_BI_04_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response: <status> 8
TC_GAW_SR_BI_05_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response: <status> 5
TC_GAW_SR_BI_06_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response: <status> 12
TC_GAW_SR_BV_05_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response:
						repeat with correct value
TC_GAW_SR_BI_07_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response
TC_GAW_SR_BI_08_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 2 <permissions> 1
				gatts start_service
TC_GAW_SR_BI_09_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response: <status> 7
TC_GAW_SR_BI_11_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response: <status> 8
TC_GAW_SR_BI_12_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response: <status> 5
TC_GAW_SR_BI_13_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response: <status> 12
TC_GAW_SR_BV_06_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
						repeat with correct value
TC_GAW_SR_BV_10_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response:
						repeat with correct value
TC_GAW_SR_BI_14_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response: <status> 1
TC_GAW_SR_BI_15_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response: <status> 3
TC_GAW_SR_BI_17_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response: <status> 8
TC_GAW_SR_BI_18_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response: <status> 5
TC_GAW_SR_BI_19_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response: <status> 12
TC_GAW_SR_BV_07_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
						repeat with correct value
TC_GAW_CL_BV_08_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response
TC_GAW_SR_BI_20_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response: <status> 1
TC_GAW_SR_BI_21_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 2 <permissions> 1
				gatts add_descriptor: <permmisions> 1
				gatts start_service
TC_GAW_SR_BI_22_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response: <status> 8

TC_GAW_SR_BI_23_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response: <status> 5
TC_GAW_SR_BI_24_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response: <status> 12
TC_GAW_SR_BV_09_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permissions> 17
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response:
						repeat with correct value
TC_GAW_SR_BI_25_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response: <status> 1
TC_GAW_SR_BI_26_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 1
				gatts start_service
TC_GAW_SR_BI_27_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 1
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response: <status> 7
TC_GAW_SR_BI_29_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response: <status> 8
TC_GAW_SR_BI_30_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response: <status> 5
TC_GAW_SR_BI_31_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response: <status> 12
TC_GAW_SR_BI_32_C	PASS	PTS issue #12823
				haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response
				gatts send_response: <status> 13
TC_GAW_SR_BI_33_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response: <status> 13
TC_GAW_SR_BI_34_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response
				gatts send_response: <status> 13
TC_GAW_SR_BI_35_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor: <permmisions> 17
				gatts start_service
				gatts send_response:
						<data> value greater than MTU
						repeat with correct offset
				gatts send_response: <status> 13
TC_GAN_CL_BV_01_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 2 0x0100
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAN_SR_BV_01_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 26 <permissions> 17
				gatts add_descriptor: <uuid> 2902
					<permission> 11
				gatts start_service
				gatts send_response
				gatts send_response
				gatts send_indication:
						<attr_handle> char value handle
						<confirm> 0
TC_GAI_CL_BV_01_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc get_descriptor <client_id> <svc_id>
					<char_id>
				gattc write_descriptor <client_id> <svc_id>
					<desc_id> 2 0x0200
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAI_SR_BV_01_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 42 <permissions> 17
				gatts add_descriptor: <permissions> 17
				gatts start_service
				gatts add_service
				gatts start_service
TC_GAS_CL_BV_01_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GAS_SR_BV_01_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 42 <permissions> 17
				gatts add_descriptor: <permissions> 17
				gatts start_service
				gatts add_service
				gatts start_service
TC_GAT_CL_BV_01_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_characteristic <conn_id> <svc_id>
					<char_id>
				wait for 30 sec timeout
TC_GAT_CL_BV_02_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc write_characteristic <client_id> <svc_id>
					<char_id> 2 <value>
				wait for 30 sec timeout
TC_GAT_SR_BV_01_C	PASS	haltest:
				gatts add_service
				gatts add_characteristic:
						<properties> 42 <permissions> 17
				gatts add_descriptor: <permissions> 17
				gatts start_service
				gatts add_service
				gatts start_service
TC_GPA_CL_BV_01_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GPA_CL_BV_02_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GPA_CL_BV_03_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GPA_CL_BV_04_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GPA_CL_BV_05_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GPA_CL_BV_06_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc connect <client id> <PTS addr>
				gattc search_service <conn_id>
				gattc get_characteristic <conn_id> <svc uuid>
				gattc read_descriptor <conn_id> <svc_id>
					<char_id> <desc_id>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GPA_CL_BV_07_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GPA_CL_BV_08_C	PASS	haltest:
				gattc connect <client id> <PTS addr>
				gattc test_command 0xe0 <PTS addr> <char_uuid>
					0x08 <start_hdl> <end_hdl>
				gattc disconnect <client_id> <PTS addr>
					<conn_id>
TC_GPA_CL_BV_11_C	PASS	haltest:
				gattc connect
				Repeat following steps 5 times:
				1.Find Characteristic Aggregate Format
				gattc test_command <cmd> 224 [u1] 8
				2.Read aggregate descriptor
				gattc test_command <cmd> 224 [u1] 10
				3.Read 3 handles from aggregate descriptor
									value
				gattc test_command <cmd> 224 [u1] 10
				4.Compare descriptors values
				gattc disconnect

TC_GPA_CL_BV_12_C	PASS	haltest:
				gattc connect
				Repeat following steps 5 times:
				1.Find Characteristic Presentation Format
				gattc test_command <cmd> 224 [u1] 8
				2.Find characteristic in this range
				gattc test_command <cmd> 224 <uuid> 2803 [u1] 8
				3.Read characteristic declaration
				gattc test_command <cmd> 224 [u1] 10
				4.Read characteristic value
				gattc test_command <cmd> 224 [u1] 10
				5.Compare characteristic value and
							presentation format
				gattc disconnect
TC_GPA_SR_BV_01_C	PASS
TC_GPA_SR_BV_02_C	PASS	haltest:
				gatts add_service
				gatts start_service
TC_GPA_SR_BV_03_C	PASS	haltest:
				gatts add_service
				gatts add_service
				add_included_service
				gatts start_service
				gatts start_service
TC_GPA_SR_BV_04_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 10 <permissions> 17
				gatts start_service
TC_GPA_SR_BV_05_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 138 <permissions> 17
				gatts add_descriptor <UUID> 2900
				gatts start_service
TC_GPA_SR_BV_06_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 138 <permissions> 17
				gatts add_descriptor <UUID> 2901
				gatts start_service
TC_GPA_SR_BV_07_C	PASS
TC_GPA_SR_BV_08_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 138 <permissions> 17
				gatts add_descriptor <UUID> 2903
				gatts start_service
				gatts send_response
TC_GPA_SR_BV_11_C	INC	PTS issue #13392
				haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 138 <permissions> 17
				gatts add_descriptor <UUID> 2905
				gatts start_service
				gatts send_response: repeat with correct offset
								and data
TC_GPA_SR_BV_12_C	PASS	haltest:
				gatts add_service
				gatts add_chaaracteristic:
						<properties> 10 <permissions> 17
				gatts add_descriptor <UUID> 2904
				gatts start_service
				gatts send_response: repeat with correct data
-------------------------------------------------------------------------------
