RFCOMM PIXIT for the PTS tool.

PTS version: 6.1

* - different than PTS defaults
& - should be set to IUT Bluetooth address
# - should be set to PTS's bin/audio folder

		Required PIXIT settings
-------------------------------------------------------------------------------
Parameter Name				Value
-------------------------------------------------------------------------------
TSPX_bd_addr_iut			11223344556677 (*&)
TSPX_delete_link_key			FALSE
TSPX_pin_code				1234
TSPX_security_enabled			TRUE
TSPX_time_guard				300000
TSPX_use_implicit_send			TRUE
TSPX_service_name_tester		COM5
TSPX_class_of_device_tester		200408
TSPX_server_channel_iut			01 (*)
TSPX_verification_pattern_length	4
TSPX_T1_Acknowledgement_Timer		20000
TSPX_T1_Acknowledgement_Timer_Dlc	300000
TSPX_T2_Response_Timer			20000
TSPX_max_frame_size_iut			127
TSPX_RPN_parameters_iut			0302001113
-------------------------------------------------------------------------------
