SDP PIXIT for the PTS tool.

PTS version: 6.1

* - different than PTS defaults
& - should be set to IUT Bluetooth address
^ - should be set accordingly
# - should be set according to the reported phone number's type

		Required PIXIT settings
-------------------------------------------------------------------------------
Parameter Name							Value
-------------------------------------------------------------------------------
TSPX_sdp_service_search_pattern					0100
TSPX_sdp_service_search_pattern_no_results			EEEE
TSPX_sdp_service_search_additional_protocol_descriptor_list
TSPX_sdp_service_search_bluetooth_profile_descriptor_list
TSPX_sdp_service_search_pattern_browse_group_list
TSPX_sdp_service_search_pattern_client_exe_url
TSPX_sdp_service_search_pattern_documentation_url
TSPX_sdp_service_search_pattern_icon_url
TSPX_sdp_service_search_pattern_language_base_attribute_id_list
TSPX_sdp_service_search_pattern_protocol_descriptor_list
TSPX_sdp_service_search_pattern_provider_name
TSPX_sdp_service_search_pattern_service_availability
TSPX_sdp_service_search_pattern_service_data_base_state		1000(*)
TSPX_sdp_service_search_pattern_service_description
TSPX_sdp_service_search_pattern_service_id
TSPX_sdp_service_search_pattern_service_info_time_to_live
TSPX_sdp_service_search_pattern_version_number_list		1000(*)
TSPX_sdp_service_search_pattern_service_name
TSPX_sdp_service_search_pattern_service_record_state
TSPX_sdp_unsupported_attribute_id				EEEE
TSPX_security_enabled						FALSE
TSPX_delete_link_key						FALSE
TSPX_bd_addr_iut						112233445566(*&)
TSPX_class_of_device_pts					200404
TSPX_class_of_device_test_pts_initiator				TRUE
TSPX_limited_inquiry_used					FALSE
TSPX_pin_code							0000
TSPX_time_guard							200000
TSPX_device_search_time						20
TSPX_use_implicit_send						TRUE
TSPX_secure_simple_pairing_pass_key_confirmation		FALSE
-------------------------------------------------------------------------------
