DID PIXIT for the PTS tool.

PTS version: 6.1

* - different than PTS defaults
& - should be set to IUT Bluetooth address

		Required PIXIT settings
-------------------------------------------------------------------------------
Parameter Name						Value
-------------------------------------------------------------------------------
TSPX_security_enabled					False
TSPX_ClientExecutableURL				False (*)
TSPX_ServiceDescription					False (*)
TSPX_DocumentationURL					False (*)
TSPX_bd_addr_iut					112233445566 (*&)
TSPX_class_of_device_pts				200404
TSPX_device_search_time					30
TSPX_delete_link_key					False
TSPX_pin_code						0000
TSPX_time_guard						200000
TSPX_use_implicit_send					True
TSPX_secure_simple_pairing_pass_key_confirmation	False
-------------------------------------------------------------------------------
