Main Page Class Hierarchy Data Structures File List Data Fields Globals

# pv_2way_h324m_types.h File Reference

`#include "pv_2way_basic_types.h"`
`#include "pv_uuid.h"`
`#include "pv_interface.h"`
`#include "pvt_common.h"`

Go to the source code of this file.

## Data Structures
class | CPVLogicalChannelIndication
class | CPVUserInput
class | CPVUserInputAlphanumeric
class | CPVUserInputDtmf
class | CPVVideoSpatialTemporalTradeoff
class | PV2Way324ConnectOptions
class | PV2Way324InitInfo
class | PVH223Al1Config
class | PVH223Al2Config
class | PVH223Al3Config
class | PVH223AlConfig
## Defines
#define | PV_2WAY_MAX_USER_INPUT_FORMATS 4
#define | PV_2WAY_MAX_SKEW_MS 1000
## Typedefs
typedef enum TPVPostDisconnectOption | PV2WayPostDisconnectOption
typedef enum UserInputType | PV2WayUserInputType
## Enumerations
enum | TPVPostDisconnectOption { EDisconnectLine, EAnalogueTelephony }
enum | UserInputType { PV_ALPHANUMERIC = 0, PV_DTMF }

## Define Documentation

#define PV_2WAY_MAX_SKEW_MS 1000

| The maximum skew that can be taken into account for both outgoing and incoming sides *

#define PV_2WAY_MAX_USER_INPUT_FORMATS 4

| The maximum number of supported formats for user input *

## Typedef Documentation

typedef enum TPVPostDisconnectOption PV2WayPostDisconnectOption

| TPVPostDisconnectOption Enum TPVPostDisconnectOption emumerates the mode the peer wants to transition to after the disconnect

typedef enum UserInputType PV2WayUserInputType

| UserInputType enum Enumeration of user input types

## Enumeration Type Documentation

enum TPVPostDisconnectOption

  | TPVPostDisconnectOption Enum TPVPostDisconnectOption emumerates the mode the peer wants to transition to after the disconnect Enumeration values:
  EDisconnectLine |
  EAnalogueTelephony |

enum UserInputType

  | UserInputType enum Enumeration of user input types Enumeration values:
  PV_ALPHANUMERIC |
  PV_DTMF |