#Test Case Name - This should be at the start
Name TestCase7

# Terminal Setup
# These setings configure how the terminal will be setup
# There are seperate settings for terminal A and Terminal B
# Settings set here do no require the full set
# Default settings will be set on the terminal. The settings explictly set here
# will override the default settings of the terminal
# Terminal A 
Terminal A
MSD undef
# capabilties
Caps
# Receive Caps
Receive
# Audio OLC caps
Audio 
AMR
G7321
# Video OLC caps
Video 
H.263BL
MP4SP
# Send Caps
Send
# Audio
Audio
AMR
G7321
# Video
Video
H.263BL
Mp4SP
#- This is not supported as of now
BER bit error injection 

#Terminal B
Terminal B
MSD undef
# capabilties
Caps
# Receive Caps
Receive
# Audio OLC caps
Audio 
AMR
G7321
# Video OLC caps
Video 
H.263BL
MP4SP
# Send Caps
Send
# Audio
Audio
AMR
G7321
# Video
Video
H.263BL
Mp4SP
#- This is not supported as of now
BER bit error injection 

# Specify the actions to be performed
# Specify the Expected behaviour

# 1. Selection of H.223 Annex B at both terminals
# 2. NSRP + CCSRL is used
# 3. RespMsg_terminalCapabilitySetAck received

