#Test Case Name - This should be at the start
Name TestCase1

# Terminal Setup
# These setings configure how the terminal will be setup
# There are seperate settings for terminal A and Terminal B
# Settings set here do no require the full set
# Default settings will be set on the terminal. The settings explictly set here
# will override the default settings of the terminal
# Terminal A 
Terminal A
H.223Muxlevel 2
# Any AL option specified here will override all the al options in the default 
# setting
AL Video
# only want to use AL3 => turn AL2 off.
AL2USE off
# Audio - use defaults
MSD undef
#- This is not supported as of now
BER bit error injection 

#Terminal B
Terminal B
H.223Muxlevel 2
# Any AL option specified here will override all the al options in the default 
# setting
AL Video
# only want to use AL3 => turn AL2 off.
AL2USE off
# Audio - use defaults
MSD undef
#- This is not supported as of now
BER bit error injection 

# Specify the actions to be performed
# Specify the Expected behaviour

# 1. Selection of H.223 Annex B at both terminals
# 2. NSRP + CCSRL is used
# 3. RespMsg_terminalCapabilitySetAck received

