# This is a sample template for the Default Settings
####################################################

# Terminal Setup
# These settings configure how the terminal will be setup
# There are separate settings for terminal A and Terminal B
# Settings set here do no require the full set
# Default settings will be set on the terminal. The settings explicitly set here
# will override the default settings of the engine and will be overridden by
# the test case file settings
# Terminal A 
Terminal A
# Set the starting level - The highest level
# The final level that is negotiated will depend on the starting level of the peer
# Annex B with Header
H.223Muxlevel 2
# Video AL'S supported
AL Video
AL3ALLOW on
AL2ALLOW on
AL1ALLOW off
# Audio ALS supported
AL Audio
AL3ALLOW off
AL2ALLOW on
AL1ALLOW off
# The SDU sizes
MaxSDUSize
AL3ALLOW 1024
AL2ALLOW 1024
# MSD Determination 
# Master indicates terminal should be master
# Slave indicates terminal should be slave
# undef indicates this is not defined and msd happens as specified in the standard
MSD undef
# capabilties
Caps Receive
# Audio OLC caps
Audio 
AMR
# Video OLC caps
Video 
MP4SP
H.263BL
# Send Caps
Caps Send
# Audio
Audio
AMR
# Video
Video
MP4SP
H.263BL

# H.263P3 - Is this supported

# Terminal B 
Terminal B
# Set the starting level - The highest level
# The final level that is negotiated will depend on the starting level of the peer
# Annex B with Header
H.223Muxlevel 2
# Video ALS supported
AL Video
AL3ALLOW on
AL2ALLOW on
AL1ALLOW off
# Audio ALS supported
AL Audio
AL3ALLOW off
AL2ALLOW on
AL1ALLOW off
# The SDU sizes
MaxSDUSize
AL3ALLOW 1024
AL2ALLOW 1024
# MSD Determination
MSD undef
# capabilties
# Receive Caps
Caps Receive
# Audio OLC caps
Audio 
AMR
# Video OLC caps
Video 
MP4SP
H.263BL
# Send Caps
Caps Send
# Audio
Audio
AMR
# Video
Video 
MP4SP
H.263BL

# H.263P3 - Is this supported