# mrcImageFFT

## Usage

    Usage: mrcImageFFT
    Options:
        [-i[nput]            In                  (NULL      ).as(inFile              ) ] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      ).as(outFile             ) ] :Essential :OutputDataFile
        [-cuda               cudaDeviceID        (0         ).as(Integer             ) ] :Optional  :UseCUDA
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         ).as(Integer             ) ] :Optional  :Mode
    ----- Additional Usage -----
    x, y and z must be even pixels.
    Excepts for like that
    (x, y, z)=(100, 1, 1)