# mrcRefFFTConvert

## Usage

    Usage: mrcRefFFTConvert
    Options:
        [-i[nput]            In                  (NULL      ).as(inFile              ) ] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      ).as(outFile             ) ] :Essential :OutputDataFile
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         ).as(Integer             ) ] :Optional  :Mode 0:Fourier translation  1:Create Fourier phase image
        [-p[ower]            Power               (1         ).as(Real                ) ] :Optional  :For mode 1 only: Use F/( |F|^p ) to create fourier phase image