# mrcImageMontageCreate

## Usage

    Usage: mrcImageMontageCreate
    Options:
        [-i[nput]            In                  (NULL      ).as(inFileListNoOpen    ) ] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      ).as(outFile             ) ] :Essential :OutputDataFile
        [-nx                 Nx                  (10        ).as(Integer             ) ] :Optional  :Nx: If this option does not set, the default value will be set
        [-ny                 Ny                  (10        ).as(Integer             ) ] :Optional  :Ny: If this option does not set, the value will be set automatically
        [-W[idth]            Width               (10        ).as(Integer             ) ] :Optional  :Width: If this option does not set, the value will be set automatically
        [-H[eight]           Height              (10        ).as(Integer             ) ] :Optional  :Height: If this option does not set, the value will be set automatically
        [-AW[indow]          AvgWnd              (2000      ).as(Real                ) ] :Optional  :AverageWindow for Pad
        [-V[alue]            Value               (0.0       ).as(Real                ) ] :Optional  :
        [-P[ad]M[ode]        PadMode             (3         ).as(Integer             ) ] :Optional  :
        [-EdgeAverage                                                                  ] :Optional  :
        [-EdgeAverageWindow  EdgeAverageWindow   (4         ).as(Integer             ) ] :Optional  :Definition of Edge
        [-NoAverage                                                                    ] :Optional  :
        [-Max                Max                 (16383     ).as(Real                ) ] :Optional  :MaximumValue: If the pixel value is more than this max, the pixel value is assigned to the Value indicated by -V or -VMax.
        [-VMax               VMax                (16383     ).as(Real                ) ] :Optional  :Attention: related to -Max
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         ).as(Integer             ) ] :Optional  :Mode
    ----- Additional Usage -----
    >>> -i inputfile <<<: InputFile Format
    hf0000.roi
    hf0001.roi
    ..........
    hf000n.roi
    >>> output file sequence <<<
    from bottom left
    >>> Pad Mode <<<
    see mrcImagePad