# mrcImageCenterGet

## Usage

    Usage: mrcImageCenterGet
    Options:
        [-i[nput]            In                  (NULL      ).as(inFile              ) ] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      ).as(outFile             ) ] :Essential :OutputDataFile
        [-Nx[Number of x]    Nx                  (0         ).as(Integer             ) ] :Optional  :Nx:Default Nx of inputfile
        [-Ny[Number of y]    Ny                  (0         ).as(Integer             ) ] :Optional  :Ny:Default Ny of inputfile
        [-Nz[Number of z]    Nz                  (0         ).as(Integer             ) ] :Optional  :Nz:Default Nz of inputfile
        [-Cx[Center x]       Cx                  (0         ).as(Real                ) ] :Optional  :Cetnter x position of extracted image.Default is center of iuput image.
        [-Cy[Center y]       Cy                  (0         ).as(Real                ) ] :Optional  :Cetnter y position of extracted image.Default is center of iuput image.
        [-Cz[Center z]       Cz                  (0         ).as(Real                ) ] :Optional  :Cetnter z position of extracted image.Default is center of iuput image.
        [-even                                                                         ] :Optional  :all dimensions of N are even.
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         ).as(Integer             ) ] :Optional  :Mode
        [-M[ode2]            mode2               (0         ).as(Integer             ) ] :Optional  :Mode2