# mrcImageGaussDisc

## Usage

    Usage: mrcImageGaussDisc
    Options:
        [-o[utput]           Out                 (NULL      ).as(outFile             ) ] :Essential :OutputDataFile
        [-sigmax             sigmax              (10        ).as(Real                ) ] :Optional  :sigmax[A]
        [-sigmay             sigmay              (10        ).as(Real                ) ] :Optional  :sigmay[A]
        [-sigma_range        sigma_range         (3         ).as(Real                ) ] :Optional  :sigma
        [-weight             weight              (10        ).as(Real                ) ] :Optional  :weight
        [-size               size                (5         ).as(Real                ) ] :Optional  :Pixel Size[A]
        [-W[idth]            Width               (0         ).as(Real                ) ] :Optional  :Image Width[A]
        [-H[eight]           Height              (0         ).as(Real                ) ] :Optional  :Image Height[A]
        [-cx                 centrex             (0         ).as(Real                ) ] :Optional  :x: Centre[A]
        [-cy                 centrey             (0         ).as(Real                ) ] :Optional  :y: Centre[A]
        [-a[ngle]            Angle               (0         ).as(Real                ) ] :Optional  :Angle: [degree]
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-m[ode]             mode                (2         ).as(Integer             ) ] :Optional  :Mode
    ----- Additional Usage -----
    Gauss Disc is cutted at sigma_range*sigma
    Gauss Disc = weight * exp ( - ((x^2 / sigmax^2)+(y^2 / sigmay^2))
    mrcImageFileSize is (sigma_range*sigmax*2) x (sigma_range*sigmay*2)
    -----------------------------------------------------------------------------------
    mode 0 char
    mode 2 float