# eosPointPositionCorrection

## Usage

    Usage: eosPointPositionCorrection
    Options:
        [-i[nput]            In                  (NULL      ).as(inFile::eosPoint    ) ] :Essential :Input:eosPoint
        [-i[nput]t[ype]      InType              (0         ).as(Integer             ) ] :Optional  :Input:eosPointMode
        [-n[umber]           N                   (-1        ).as(Integer             ) ] :Optional  :Input:number of Point, n, dependent upon m=n/(n-1)/2, a point number in In
        [-o[utput]           Out                 (stdout    ).as(outFile::eosPoint   ) ] :Optional  :Output:eosPoint
        [-o[utput]t[ype]     OutType             (0         ).as(Integer             ) ] :Optional  :Output:eosPoint
        [-delta              OutDelta            (stdout    ).as(outFile::eosPoint   ) ] :Optional  :Output:eosPoint
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         ).as(Integer             ) ] :Optional  :Mode
    ----- Additional Usage -----
    type-0: x y z
    type-1: x y z sig
    type-2: x y z sigx sigy sigz
    type-3: x y z sig sigx sigy sigz