# mrcFFTProjection

## Usage

    Usage: mrcFFTProjection
    Options:
        [-i[nput]            In                  (NULL      ).as(inFile              ) ] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      ).as(outFile             ) ] :Essential :OutputDataFile
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         ).as(Integer             ) ] :Optional  :Mode
    ----- Additional Usage -----
    The 2D FFT Image projects to Y-axis
    This image is not true.
    Because the real part is buried with mag and the imaginary part is buried with zero.