-----BEGIN PGP SIGNED MESSAGE-----

First:

    HiSax is free software; you can redistribute it and/or modify
    it under the terms of the GNU General Public License as published by
    the Free Software Foundation; either version 2 of the License, or
    (at your option) any later version.

    This program is distributed in the hope that it will be useful,
    but WITHOUT ANY WARRANTY; without even the implied warranty of
    MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
    GNU General Public License for more details.

However, if you wish to modify the HiSax sources, please note the following:

HiSax has passed the ITU approval test suite with ELSA Quickstep ISDN cards
and Eicon Technology Diva 2.01 PCI card.
The certification is only valid for the combination of the tested software
version and the tested hardware. Any changes to the HiSax source code may
therefore affect the certification.

Additional ITU approval tests have been carried out for all generic cards
using Colognechip single chip solutions HFC-S PCI A for PCI cards as well
as HFC-S USB based USB ISDN ta adapters.
These tests included all layers 1-3 and as well all functional tests for 
the layer 1. Because all hardware based on these chips are complete ISDN
solutions in one chip all cards and USB-TAs using these chips are to be
regarded as approved for those tests. Some additional electrical tests
of the layer 1 which are independant of the driver and related to a
special hardware used will be regarded as approved if at least one 
solution has been tested including those electrical tests. So if cards 
or tas have been completely approved for any other os, the approval
for those electrical tests is valid for linux, too.
Please send any questions regarding this drivers or approval abouts to 
werner@isdn-development.de 
Additional information and the type approval documents will be found
shortly on the Colognechip website www.colognechip.com 

If you change the main files of the HiSax ISDN stack, the certification will
become invalid. Because in most countries it is illegal to connect
unapproved ISDN equipment to the public network, I have to guarantee that
changes in HiSax do not affect the certification.

In order to make a valid certification apparent to the user, I have built in
some validation checks that are made during the make process. The HiSax main
files are protected by md5 checksums and the md5sum file is pgp signed by
myself:

KeyID 1024/FF992F6D 1997/01/16 Karsten Keil <kkeil@suse.de>
Key fingerprint = 92 6B F7 58 EE 86 28 C8  C4 1A E6 DC 39 89 F2 AA

Only if the checksums are OK, and the signature of the file
"drivers/isdn/hisax/md5sums.asc" match, is the certification valid; a
message confirming this is then displayed during the hisax init process.

The affected files are:

drivers/isdn/hisax/isac.c
drivers/isdn/hisax/isdnl1.c
drivers/isdn/hisax/isdnl2.c
drivers/isdn/hisax/isdnl3.c
drivers/isdn/hisax/tei.c
drivers/isdn/hisax/callc.c
drivers/isdn/hisax/l3dss1.c
drivers/isdn/hisax/l3_1tr6.c
drivers/isdn/hisax/cert.c
drivers/isdn/hisax/elsa.c
drivers/isdn/hisax/diva.c
drivers/isdn/hisax/hfc_pci.c

Please send any changes, bugfixes and patches to me rather than implementing
them directly into the HiSax sources.

This does not reduce your rights granted by the GNU General Public License.
If you wish to change the sources, go ahead; but note that then the
certification is invalid even if you use one of the approved cards.

Here are the certification registration numbers for ELSA Quickstep cards:
German   D133361J CETECOM ICT Services GmbH 0682
European D133362J CETECOM ICT Services GmbH 0682


Karsten Keil
keil@isdn4linux.de

-----BEGIN PGP SIGNATURE-----
Version: 2.6.3i
Charset: noconv

iQCVAwUBOFAwqTpxHvX/mS9tAQFI2QP9GLDK2iy/KBhwReE3F7LeO+tVhffTVZ3a
20q5/z/WcIg/pnH0uTkl2UgDXBFXYl45zJyDGNpAposIFmT+Edd14o7Vj1w/BBdn
Y+5rBmJf+gyBu61da5d6bv0lpymwRa/um+ri+ilYnZ/XPfg5JKhdjGSBCJuJAElM
d2jFbTrsMYw=
=LNf9
-----END PGP SIGNATURE-----
