--- Configure.help-2.4.7	2001/12/20 11:38:45	1.1.1.8
+++ Configure.help-2.4.8	2001/12/20 11:39:06	1.1.1.9
@@ -3245,6 +3245,18 @@
   module will be called atyfb.o. If you want to compile it as a
   module, say M here and read Documentation/modules.txt.
   
+ATI Mach64 GX display support (EXPERIMENTAL)
+CONFIG_FB_ATY_GX
+  This options adds support for the first generation ATI Mach64
+  graphics chips, i.e. the Mach64 GX and CX. Note that this support is
+  limited.
+
+ATI Mach64 CT/VT/GT/LT display support (EXPERIMENTAL)
+CONFIG_FB_ATY_CT
+  This option adss support for ATI Mach64 graphics chips starting
+  with the Mach64 CT family. This includes the Mach64 VT (limited
+  support), GT (3D RAGE family), and LT.
+
 ATI Rage128 display support (EXPERIMENTAL)
 CONFIG_FB_ATY128
   This driver supports graphics boards with the ATI Rage128 chips.
@@ -12471,6 +12483,33 @@
   Say Y here if you would like to use hard disks under Linux which
   were partitioned on a Macintosh.
 
+Windows' Logical Disk Manager (Dynamic Disk) support (EXPERIMENTAL)
+CONFIG_LDM_PARTITION
+  Say Y here if you would like to use hard disks under Linux which
+  were partitioned using Windows 2000's or XP's Logical Disk Manager.
+  They are also known as "Dynamic Disks".
+
+  Windows 2000 introduced the concept of Dynamic Disks to get around
+  the limitations of the PC's partitioning scheme.  The Logical Disk
+  Manager allows the user to repartion a disk and create spanned,
+  mirrored, striped or RAID volumes, all without the need for
+  rebooting.
+
+  Normal partitions are now called Basic Disks under Windows 2000 and XP.
+
+  Technical documentation to accompany this driver is available from:
+  <http://linux-ntfs.sf.net/ldm>
+
+  If unsure, say N.
+
+Windows' LDM extra logging
+CONFIG_LDM_DEBUG
+  Say Y here if you would like LDM to log verbosely.  This could be
+  helpful if the driver doesn't work as expected and you'd like to
+  report a bug.
+
+  If unsure, say N.
+
 PC BIOS (MSDOS partition tables) support
 CONFIG_MSDOS_PARTITION
   Say Y here if you would like to use hard disks under Linux which
@@ -14201,6 +14240,19 @@
 
   If unsure, say N.
 
+Sony Vaio Programmable I/O Control Device support
+CONFIG_SONYPI
+  This driver enables access to the Sony Programmable I/O Control Device
+  which can be found in many (all ?) Sony Vaio laptops.
+
+  If you have one of those laptops, read Documentation/sonypi.txt,
+  and say Y or M here.
+
+  If you want to compile the driver as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want),
+  say M here and read <file:Documentation/modules.txt>. The module will be
+  called sonypi.o.
+
 Intel Random Number Generator support
 CONFIG_INTEL_RNG
   This driver provides kernel-side support for the Random Number
@@ -17493,6 +17545,19 @@
   module called pms.o ( = code which can be inserted in and removed
   from the running kernel whenever you want). If you want to compile
   it as a module, say M here and read Documentation/modules.txt.
+
+CONFIG_VIDEO_MEYE
+  This is the video4linux driver for the Motion Eye camera found
+  in the Vaio Picturebook laptops. Please read the material in
+  <file:Documentation/video4linux/meye.txt> for more information.
+
+  If you say Y or M here, you need to say Y or M to "Sony Programmable
+  I/O Control Device" in the character device section.
+
+  This driver is available as a module called meye.o ( = code
+  which can be inserted in and removed from the running kernel
+  whenever you want). If you want to compile it as a module, say M
+  here and read <file:Documentation/modules.txt>.
 
 IBM's S/390 architecture
 CONFIG_ARCH_S390
