--- Configure.help-2.4.13	2001/12/20 11:41:52	1.1.1.13
+++ Configure.help-2.4.14	2001/12/20 11:42:19	1.1.1.14
@@ -1412,6 +1412,12 @@
   have a high-level driver for the type of device that you want to
   support.
 
+Shuttle EPAT c7/c8 extension 
+CONFIG_PARIDE_EPATC8
+  This option enables support for the newer Shuttle EP1284 (aka c7 and
+  c8) chip. You need this if you are using any recent Imation SuperDisk
+  (LS-120) drive.
+
 Shuttle EPIA protocol
 CONFIG_PARIDE_EPIA
   This option enables support for the (obsolete) EPIA parallel port
@@ -1934,6 +1940,20 @@
   If you want to compile it as a module, say M here and read
   Documentation/modules.txt.  If unsure, say `N'.
 
+IRC Send/Chat support
+CONFIG_IP_NF_IRC
+  There is a commonly-used extension to IRC called
+  Direct Client-to-Client Protocol (DCC).  This enables users to send
+  files to each other, and also chat to each other without the need
+  of a server.  DCC Sending is used anywhere you send files over IRC,
+  and DCC Chat is most commonly used by Eggdrop bots.  If you are
+  using NAT, this extension will enable you to send files and initiate
+  chats.  Note that you do NOT need this extension to get files or
+  have others initiate chats, or everything else in IRC.
+
+  If you want to compile it as a module, say 'M' here and read
+  Documentation/modules.txt.  If unsure, say 'N'.
+
 FTP protocol support
 CONFIG_IP_NF_FTP
   Tracking FTP connections is problematic: special helpers are
@@ -1960,7 +1980,41 @@
 
   If you want to compile it as a module, say M here and read
   Documentation/modules.txt.  If unsure, say `N'.
+CONFIG_IP6_NF_MATCH_LIMIT
+  limit matching allows you to control the rate at which a rule can be
+  matched: mainly useful in combination with the LOG target ("LOG
+  target support", below) and to avoid some Denial of Service attacks.
+
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt.  If unsure, say `N'.
+
+MAC address match support
+CONFIG_IP6_NF_MATCH_MAC
+  mac matching allows you to match packets based on the source
+  ethernet address of the packet.
 
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt.  If unsure, say `N'.
+
+Multiple port match support
+CONFIG_IP6_NF_MATCH_MULTIPORT
+  Multiport matching allows you to match TCP or UDP packets based on
+  a series of source or destination ports: normally a rule can only
+  match a single range of ports.
+
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt.  If unsure, say `N'.
+
+Owner match support (EXPERIMENTAL)
+CONFIG_IP6_NF_MATCH_OWNER
+  Packet owner matching allows you to match locally-generated packets
+  based on who created them: the user, group, process or session.
+
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt.  If unsure, say `N'.
+
+
+
 limit match support
 CONFIG_IP_NF_MATCH_LIMIT
   limit matching allows you to control the rate at which a rule can be
@@ -1996,6 +2050,22 @@
   If you want to compile it as a module, say M here and read
   Documentation/modules.txt.  If unsure, say `N'.
 
+TTL match support
+CONFIG_IP_NF_MATCH_TTL
+  This adds CONFIG_IP_NF_MATCH_TTL option, which enabled the user
+  to match packets by their TTL value.
+
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt.  If unsure, say `N'.
+
+length match support
+CONFIG_IP_NF_MATCH_LENGTH
+  This option allows you to match the length of a packet against a
+  specific value or range of values.
+
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt.  If unsure, say `N'.
+
 TOS match support
 CONFIG_IP_NF_MATCH_TOS
   TOS matching allows you to match packets based on the Type Of
@@ -2075,6 +2145,20 @@
   If you want to compile it as a module, say M here and read
   Documentation/modules.txt.  If unsure, say `N'.
 
+Basic SNMP-ALG support
+CONFIG_IP_NF_NAT_SNMP_BASIC
+
+  This module implements an Application Layer Gateway (ALG) for 
+  SNMP payloads.  In conjunction with NAT, it allows a network 
+  management system to access multiple private networks with 
+  conflicting addresses.  It works by modifying IP addresses 
+  inside SNMP payloads to match IP-layer NAT mapping.
+  
+  This is the "basic" form of SNMP-ALG, as described in RFC 2962
+  
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt.  If unsure, say `N'.
+
 REDIRECT target support
 CONFIG_IP_NF_TARGET_REDIRECT
   REDIRECT is a special case of NAT: all incoming connections are
@@ -2215,6 +2299,14 @@
   If you want to compile it as a module, say M here and read
   Documentation/modules.txt.  If unsure, say `N'.
 
+LOG target support
+CONFIG_IP6_NF_TARGET_LOG
+  This option adds a `LOG' target, which allows you to create rules in
+  any ip6tables table which records the packet header to the syslog.
+
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt.  If unsure, say `N'.
+
 Packet filtering
 CONFIG_IP6_NF_FILTER
   Packet filtering defines a table `filter', which has a series of
@@ -11142,7 +11234,7 @@
   mice, joysticks, graphic tablets, or any other HID based devices
   to your computer via USB. You can't use this driver and the
   HIDBP (Boot Protocol) keyboard and mouse drivers at the same time.
-  More information is available: Documentation/usb/input.txt.
+  More information is available: Documentation/input/input.txt.
 
   If unsure, say Y.
 
@@ -12166,6 +12258,15 @@
   http://www.unicode.org for more information). Say Y here if you want
   to be able to read Joliet CDROMs under Linux.
 
+Transparent decompression extension
+CONFIG_ZISOFS
+  This is a Linux-specific extension to RockRidge which lets you store
+  data in compressed form on a CD-ROM and have it transparently
+  decompressed when the CD-ROM is accessed.  See
+  <http://www.kernel.org/pub/linux/utils/fs/zisofs/> for the tools
+  necessary to create such a filesystem.  Say Y here if you want to be
+  able to read such compressed CD-ROMs.
+
 UDF File System support (read only)
 CONFIG_UDF_FS
   This is the new file system used on some CDROMs and DVDs. Say Y if
@@ -14948,6 +15049,25 @@
   http://www.buzzard.org.uk/toshiba/
 
   Say Y if you intend to run this kernel on a Toshiba portable.
+  Say N otherwise.
+
+Dell Inspiron 8000 support
+CONFIG_I8K
+  This adds a driver to safely access the System Management Mode
+  of the CPU on the Dell Inspiron 8000. The System Management Mode
+  is used to read cpu temperature and cooling fan status and to
+  control the fans on the I8K portables.
+
+  This driver has been tested only on the Inspiron 8000 but it may
+  also work with other Dell laptops. You can force loading on other
+  models by passing the parameter `force=1' to the module. Use at
+  your own risk.
+
+  For information on utilities to make use of this driver see the
+  I8K Linux utilities web site at:
+  http://www.debian.org/~dz/i8k/
+
+  Say Y if you intend to run this kernel on a Dell Inspiron 8000.
   Say N otherwise.
 
 /dev/cpu/microcode - Intel IA32 CPU microcode support
