--- Configure.help-2.4.36	2008-01-16 12:30:08.000000000 +0900
+++ Configure.help-2.4.37	2008-12-08 22:48:04.000000000 +0900
@@ -3211,0 +3212,11 @@
+CLASSIFY target support
+CONFIG_IP_NF_TARGET_CLASSIFY
+  This option adds a `CLASSIFY' target, which enables the user to set
+  the priority of a packet. Some qdiscs can use this value for classification,
+  among these are:
+
+  atm, cbq, dsmark, pfifo_fast, htb, prio
+
+  If you want to compile it as a module, say M here and read
+  Documentation/modules.txt.  If unsure, say `N'.
+
@@ -4822,0 +4834 @@
+   - "Geode GX/LX" for AMD/NSC Geode GX and AMD Geode LX.
@@ -20191,0 +20204,16 @@
+AMD Geode LX HW Random Number Generator support
+CONFIG_GEODE_RNG
+  This driver provides kernel-side support for the Random Number
+  Generator hardware found on the AMD Geode LX.
+
+  It runs a timer function which automatically adds entropy directly
+  into the kernel pool. You may need this driver if your system runs
+  headless and has no other source of entropy.
+
+  To compile this driver as a module ( = code which can be inserted in
+  and removed from the running kernel whenever you want), say M here
+  and read <file:Documentation/modules.txt>. The module will be called
+  hw_random.
+
+  If unsure, say N.
+
@@ -20663,0 +20692,16 @@
+AMD/NSC Geode Hardware Watchdog
+CONFIG_GEODE_WDT
+  This driver enables a watchdog capability built into the
+  CS5535/CS5536 companion chips for the AMD Geode GX and LX
+  processors.  This watchdog watches your kernel to make sure
+  it doesn't freeze, and if it does, it reboots your computer after
+  a certain amount of time.
+
+  This driver depends on CONFIG_MGEODE_LX.
+
+  This driver is also available as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want).
+  The module is called geodewdt.o.  If you want to compile it as a
+  module, say M here and read <file:Documentation/modules.txt>.  Most
+  people will say N.
+
@@ -28810,0 +28855 @@
+  It also enables the I2C controller found on Geode GX/LX processors.
