--- Configure.help-2.4.9	2001/12/20 11:39:34	1.1.1.10
+++ Configure.help-2.4.10	2001/12/20 11:40:19	1.1.1.11
@@ -1746,6 +1746,36 @@
   similar) CPU, R4xx0 might be a safe bet.
   If the resulting Kernel does not work try to recompile with R3000.
 
+CPU type
+CONFIG_CPU_VR41XX
+  The options selects support for the NEC VR41xx series of processors.
+  Only choose this option if you have one of these processors as a
+  kernel built with this option will not run on any other type of
+  processor or vice versa.
+
+CPU feature configuration
+CONFIG_CPU_ADVANCED
+  Saying yes here allows you to select support for various features your
+  CPU may or may not have.  Most people should say N here.
+
+ll and sc instructions
+CONFIG_CPU_HAS_LLSC
+  Say Y here if your CPU has the ll and sc instructions.  Say Y here for
+  better performance, N if you don't know.  You must say Y here for
+  multiprocessor machines.
+
+lld and scd instructions
+CONFIG_CPU_HAS_LLDSCD
+  Say Y here if your CPU has the lld and scd instructions, the 64-bit
+  equivalents of ll and sc.  Say Y here for better performance, N if
+  you don't know.  You must say Y here for multiprocessor machines.
+
+Support for writebuffer flushing
+CONFIG_CPU_HAS_WB
+  Say N here for slightly better performance.  You must say Y here for
+  machines which require flushing of write buffers in software.  Saying
+  Y is the safe option; N may result in kernel malfunction and crashes.
+
 Support for large 64-bit configurations
 CONFIG_MIPS_INSANE_LARGE
   MIPS R10000 does support a 44 bit / 16TB address space as opposed to
@@ -2548,10 +2578,10 @@
   the GLX component for XFree86 3.3.6, which can be downloaded from
   http://utah-glx.sourceforge.net/ .
 
-AMD Irongate support
+AMD Irongate, 761, and 762 support
 CONFIG_AGP_AMD
   This option gives you AGP support for the GLX component of the
-  XFree86 4.x on AMD Irongate chipset.
+  XFree86 4.x on AMD Irongate, 761, and 762 chipsets.
 
   For the moment, you should probably say N, unless you want to test
   the GLX component for XFree86 3.3.6, which can be downloaded from
@@ -8779,13 +8809,13 @@
   say M here and read Documentation/modules.txt. This is recommended.
   The module will be called sis900.o.
 
-Packet Engines Yellowfin Gigabit-NIC support
+Packet Engines Yellowfin Gigabit-NIC / Symbios 53c885 support
 CONFIG_YELLOWFIN
   Say Y here if you have a Packet Engines G-NIC PCI Gigabit Ethernet
-  adapter. This adapter is used by the Beowulf Linux cluster project.
-  See http://cesdis.gsfc.nasa.gov/linux/drivers/yellowfin.html for
-  more information about this driver in particular and Beowulf in
-  general.
+  adapter or the SYM53C885 Ethernet controller. The Gigabit adapter is
+  used by the Beowulf Linux cluster project.  See
+  http://cesdis.gsfc.nasa.gov/linux/drivers/yellowfin.html for more
+  information about this driver in particular and Beowulf in general.
 
   If you want to compile this driver as a module ( = code which can be
   inserted in and removed from the running kernel whenever you want),
@@ -11220,6 +11250,17 @@
   The module will be called keyspan_pda.o. If you want to compile it 
   as a module, say M here and read Documentation/modules.txt.
 
+USB Xircom / Entregra Single Port Serial Driver
+CONFIG_USB_SERIAL_XIRCOM
+  Say Y here if you want to use a Xircom or Entregra single port USB to
+  serial converter device.  This driver makes use of firmware
+  developed from scratch by Brian Warner.
+
+  This code is also available as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want).
+  The module will be called keyspan_pda.o. If you want to compile it
+  as a module, say M here and read <file:Documentation/modules.txt>.
+
 USB Keyspan USA-xxx Serial Driver
 CONFIG_USB_SERIAL_KEYSPAN
   Say Y here if you want to use Keyspan USB to serial converter
@@ -11478,6 +11519,45 @@
   The module will be called pegasus.o. If you want to compile it as a
   module, say M here and read Documentation/modules.txt.
 
+CONFIG_USB_KAWETH
+  Say Y here if you want to use one of the following 10Mbps only
+  USB Ethernet adapters based on the KLSI KL5KUSB101B chipset:
+       3Com 3C19250
+       ADS USB-10BT
+       ATEN USB Ethernet
+       ASANTE USB To Ethernet Adapter
+       AOX Endpoints USB Ethernet
+       Correga K.K.
+       D-Link DSB-650C and DU-E10
+       Entrega / Portgear E45
+       I-O DATA USB-ET/T
+       Jaton USB Ethernet Device Adapter
+       Kingston Technology USB Ethernet Adapter
+       Linksys USB10T
+       Mobility USB-Ethernet Adapter
+        NetGear EA-101
+       Peracom Enet and Enet2
+       Portsmith Express Ethernet Adapter
+       Shark Pocket Adapter
+       SMC 2202USB
+       Sony Vaio port extender
+
+  This driver is likely to work with most 10Mbps only USB Ethernet
+  adapters, including some "no brand" devices. It does NOT work on
+  SmartBridges smartNIC or on Belkin F5U111 devices - you should use
+  the CATC NetMate driver for those. If you are not sure which one
+  you need, select both, and the correct one should be selected for
+  you.
+
+  This driver makes the adapter appear as a normal Ethernet interface,
+  typically on eth0, if it is the only ethernet device, or perhaps on
+  eth1, if you have a PCI or ISA ethernet card installed.
+
+  This code is also available as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want).
+  The module will be called kaweth.o. If you want to compile it as a
+  module, say M here and read <file:Documentation/modules.txt>.
+
 USB CATC NetMate-based Ethernet device support
 CONFIG_USB_CATC
   Say Y if you want to use one of the following 10Mbps USB Ethernet
@@ -11492,6 +11572,29 @@
   The module will be called catc.o. If you want to compile it as a
   module, say M here and read <file:Documentation/modules.txt>.
 
+USB Communication Class Ethernet driver
+CONFIG_USB_CDCETHER
+  This driver supports devices conforming to the Communication Device
+  Class Ethernet Control Model.  This is used in some cable modems.
+  For more details on the specification, get the Communication Device
+  Class specification from <http://www.usb.org>.
+
+  This driver should work with the following devices:
+        * Ericsson PipeRider (all variants)
+        * Motorola (DM100 and SB4100)
+        * Broadcom Cable Modem (reference design)
+        * Toshiba PCX1100U and possibly other cable modems
+
+  The device creates a network device (ethX, where X depends on what
+  other networking devices you have in use), as for a normal PCI
+  or ISA based ethernet network card.
+
+  This code is also available as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want).
+  The module will be called CDCEther.o.  If you want to compile it as
+  a module, say M here and read <file:Documentation/modules.txt>.
+
+
 USB Kodak DC-2xx Camera support
 CONFIG_USB_DC2XX
   Say Y here if you want to connect this type of still camera to
@@ -11532,6 +11635,20 @@
   Say Y here in order to have the USB Mass Storage code generate
   verbose debugging messages.
 
+ISD-200 USB/ATA driver
+CONFIG_USB_STORAGE_ISD200
+  Say Y here if you want to use USB Mass Store devices based
+  on the In-Systems Design ISD-200 USB/ATA bridge.
+
+  Some of the products that use this chip are:
+
+    - Archos Jukebox 6000
+    - ISD SmartCable for Storage
+    - Taiwan Skymaster CD530U/DEL-0241 IDE bridge
+    - Sony CRX10U CD-R/RW drive
+    - CyQ've CQ8060A CDRW drive
+    - Planex eXtreme Drive RX-25HU USB-IDE cable (not model RX-25U)
+
 USS720 parport driver
 CONFIG_USB_USS720
   This driver is for USB parallel port adapters that use the Lucent
@@ -11604,18 +11721,22 @@
   The module will be called dabusb.o. If you want to compile it as a
   module, say M here and read Documentation/modules.txt.
 
-PLUSB driver
-CONFIG_USB_PLUSB
-  A driver for the Prolific PL-2302 USB-to-USB network device. This
-  'USB cable' connects two hosts via a point-to-point network with
-  bandwidth of 5 Mbit/s. Configure this driver after connecting the
-  USB cable via ifconfig plusb0 10.0.0.1 pointopoint 10.0.0.2 (and
-  vice versa on the other host).
+Host-to-Host USB networking
+CONFIG_USB_USBNET
+  This driver supports network links over USB with USB "Network"
+  or "data transfer" cables, often used to network laptops to PCs.
+  Such cables have chips from suppliers such as NetChip and Prolific.
+  Intelligent USB devices could also use this approach to provide
+  Internet access, using standard USB cabling.
+
+  These links will have names like "usb0", "usb1", etc.  They act
+  like two-node Ethernets, so you can use 802.1d Ethernet Bridging
+  (CONFIG_BRIDGE) to simplify your network routing.
 
-  This code is also available as a module ( = code which can be
+  This code is also available as a kernel module (code which can be
   inserted in and removed from the running kernel whenever you want).
-  The module will be called plusb.o. If you want to compile it as a
-  module, say M here and read Documentation/modules.txt.
+  The module will be called usbnet.o. If you want to compile it as a
+  module, say M here and read <file:Documentation/modules.txt>.
 
 USB Diamond Rio500 support
 CONFIG_USB_RIO500
@@ -15754,6 +15875,14 @@
   better 32 MB RAM to avoid excessive linking time. This is only
   useful for kernel hackers. If unsure, say N.
 
+Run uncached
+CONFIG_MIPS_UNCACHED
+  If you say Y here there kernel will disable all CPU caches.  This will
+  reduce the system's performance dramatically but can help finding
+  otherwise hard to track bugs.  It can also useful if you're doing
+  hardware debugging with a logic analyzer and need to see all traffic
+  on the bus.
+
 Magic System Request Key support
 CONFIG_MAGIC_SYSRQ
   If you say Y here, you will have some control over the system even
@@ -16960,12 +17089,12 @@
 
 Motorola MPC8260 CPM support
 CONFIG_8260
-   The MPC8260 CPM (Communications Processor Module) is a typically
-   embedded CPU made by Motorola.  Selecting this option means that
-   you wish to build a kernel for a machine with specifically an 8260
-   for a CPU.
+  The MPC8260 CPM (Communications Processor Module) is a typical
+  embedded CPU made by Motorola. Selecting this option means that you
+  wish to build a kernel for a machine with specifically an 8260 for
+  a CPU.
 
-   If in doubt, say N.
+  If in doubt, say N.
 
 Workarounds for PPC601 bugs
 CONFIG_PPC601_SYNC_FIX
@@ -16983,12 +17112,191 @@
 CONFIG_ALL_PPC
   Linux currently supports several different kinds of PowerPC-based
   machines: Apple Power Macintoshes and clones (such as the Motorola
-  Starmax series), PReP (PowerPC Reference Platform) machines such as
-  the Motorola PowerStack, CHRP (Common Hardware Reference Platform), 
-  the embedded MBX boards from Motorola and many others. Currently, 
-  the default option is to build a kernel which works on the first 
-  three.  Support for other machines is currently incomplete.
+  Starmax series), PReP (PowerPC Reference Platform) machines (such
+  as the Motorola PowerStacks, Motorola cPCI/VME embedded systems,
+  and some IBM RS/6000 systems), CHRP (Common Hardware Reference
+  Platform), and several embedded PowerPC systems containing 4xx, 6xx,
+  7xx, 8xx, 74xx, and 82xx processors.  Currently, the default option
+  is to build a kernel which works on the first three. 
+
+Embedded 8xx Board Type
+CONFIG_RPXLITE
+  RPX-Lite:
+    Embedded Planet RPX Lite
+
+  RPX-Classic:
+    Embedded Planet RPX Classic Low-fat.
+
+  BSE-IP: 
+    Bright Star Engineering ip-Engine.
+
+  TQM823L:
+  TQM850L:
+  TQM855L:
+  TQM860L:
+    MPC8xx based family of mini modules, half credit card size,
+    up to 64 MB of RAM, 8 MB Flash, (Fast) Ethernet, 2 x serial ports,
+    2 x CAN bus interface, ...
+      Manufacturer: TQ Components, www.tq-group.de
+      Date of Release: October (?) 1999
+      End of Life: not yet :-)
+      URL:
+      - module: http://www.denx.de/PDF/TQM8xxLHWM201.pdf
+      - starter kit: http://www.denx.de/PDF/STK8xxLHWM201.pdf
+      - images: http://www.denx.de/embedded-ppc-en.html
+
+  FPS850L:
+    FingerPrint Sensor System (based on TQM850L)
+      Manufacturer: IKENDI AG, http://www.ikendi.com/
+      Date of Release: November 1999
+      End of life: end 2000 ?
+      URL: see TQM850L
+
+  SPD823TS:
+    MPC823 based board used in the "Tele Server" product
+    Manufacturer: Speech Design, http://www.speech-design.de/
+    Date of Release: Mid 2000 (?)
+    End of life: -
+    URL: http://www.speech-design.de/
+         select "English", then "Teleteam Solutions", then "TeleServer"
+
+  IVMS8:
+    MPC860 based board used in the "Integrated Voice Mail System",
+    Small Version (8 voice channels)
+    Manufacturer: Speech Design, http://www.speech-design.de/
+    Date of Release: December 2000 (?)
+    End of life: -
+    URL: http://www.speech-design.de/
+
+  IVML24:
+    MPC860 based board used in the "Integrated Voice Mail System", 
+    Large Version (24 voice channels)
+    Manufacturer: Speech Design, http://www.speech-design.de/
+    Date of Release: March 2001  (?)
+    End of life: -
+    URL: http://www.speech-design.de/
+
+  SM850:
+    Service Module (based on TQM850L)
+    Manufacturer: Dependable Computer Systems, http://www.decomsys.com/
+    Date of Release: end 2000 (?)
+    End of life: mid 2001 (?)
+    URL: http://www.tz-mikroelektronik.de/ServiceModule/index.html
+
+  HERMES:
+    Hermes-Pro ISDN/LAN router with integrated 8 x hub
+    Manufacturer: Multidata Gesellschaft für Datentechnik und Informatik
+      http://www.multidata.de/
+    Date of Release: 2000 (?)
+    End of life: -
+    URL: http://www.multidata.de/english/products/hpro.htm
+
+  IP860:	
+    VMEBus IP (Industry Pack) carrier board with MPC860
+    Manufacturer: MicroSys GmbH, http://www.microsys.de/
+    Date of Release: ?
+    End of life: -
+    URL: http://www.microsys.de/html/ip860.html
+
+  PCU_E:
+    PCU = Peripheral Controller Unit, Extended
+    Manufacturer: Siemens AG, ICN (Information and Communication Networks)
+    	http://www.siemens.de/page/1,3771,224315-1-999_2_226207-0,00.html
+    Date of Release: April 2001
+    End of life: August 2001
+    URL: n. a.
+
+Embedded 82xx Board Type
+CONFIG_EST8260
+  EST8260: Wind River System, Inc. EST SBC8260
+
+  TQM8260:
+    MPC8260 based module, little larger than credit card,
+    up to 128 MB global + 64 MB local RAM, 32 MB Flash,
+    32 kB EEPROM, 256 kB L@ Cache, 10baseT + 100baseT Ethernet,
+    2 x serial ports, ...
+      Manufacturer: TQ Components, www.tq-group.de
+      Date of Release: June 2001
+      End of Life: not yet :-)
+      URL: http://www.denx.de/PDF/TQM82xx_SPEC_Rev005.pdf
+
+  PM826:
+    Modular system with MPC8260 CPU
+    Manufacturer: MicroSys GmbH, http://www.microsys.de/
+    Date of Release: mid 2001
+    End of life: -
+    URL: http://www.microsys.de/html/pm826.html
+
+  CU824:
+    VMEBus Board with PCI extension with MPC8240 CPU
+    Manufacturer: MicroSys GmbH, http://www.microsys.de/
+    Date of Release: early 2001 (?)
+    End of life: -
+    URL: http://www.microsys.de/html/cu824.html
+
+AltiVec Kernel Support
+CONFIG_ALTIVEC
+  This option enables kernel support for the Altivec extensions to the
+  PowerPC processor. The kernel currently supports saving and restoring
+  altivec registers, and turning on the 'altivec enable' bit so user
+  processes can execute altivec instructions.
+
+  This option is only usefully if you have a processor that supports 
+  altivec (G4, otherwise known as 74xx series), but does not have
+  any affect on a non-altivec cpu (it does, however add code to the
+  kernel).
+
+  If in doubt, say Y here.
+
+Thermal Management Support
+CONFIG_TAU
+  G3 and G4 processors have an on-chip temperature sensor called the
+  'Thermal Assist Unit (TAU)', which, in theory, can measure the on-die
+  temperature within 2-4 degrees celcius. This option shows the current
+  on-die temperature in /proc/cpuinfo if the cpu supports it.
+
+  Unfortunately, on some chip revisions, this sensor is very inaccurate
+  and in some cases, does not work at all, so don't assume the cpu
+  temp is actually what /proc/cpuinfo says it is.
+
+Interrupt driven TAU driver
+CONFIG_TAU_INT
+  The TAU supports an interrupt driven mode which causes an interrupt
+  whenever the temperature goes out of range. This is the fastest way
+  to get notified the temp has exceeded a range. With this option off,
+  a timer is used to re-check the temperature periodically.
+
+  However, on some cpus it appears that the TAU interrupt hardware
+  is buggy and can cause a situation which would lead unexplained hard
+  lockups.
 
+  Unless you are extending the TAU driver, or enjoy kernel/hardware
+  debugging, leave this option off.
+
+Average high and low temp
+CONFIG_TAU_AVERAGE
+  The TAU hardware can compare the temperature to an upper and lower bound.
+  The default behavior is to show both the upper and lower bound in 
+  /proc/cpuinfo. If the range is large, the temperature is either changing
+  a lot, or the TAU hardware is broken (likely on some G4's). If the range
+  is small (around 4 degrees), the temperature is relatively stable.
+
+Support for CUDA based PowerMacs
+CONFIG_ADB_CUDA
+  This provides support for CUDA based Power Macintosh systems.  This
+  includes most OldWorld PowerMacs, the first generation iMacs, the
+  Blue&White G3 and the Yikes G4 (PCI Graphics).  All later models
+  should use CONFIG_ADB_PMU instead.
+
+  If unsure say Y.
+
+Support for PMU based PowerMacs
+CONFIG_ADB_PMU
+  This provides support for PMU based Power Macintosh systems.  This
+  includes all PowerBooks and all AGP-based machines.
+  
+  If unsure say Y.
+
 Power management support for PowerBooks
 CONFIG_PMAC_PBOOK
   This provides support for putting a PowerBook to sleep; it also
@@ -17005,13 +17313,6 @@
   have it autoloaded. The act of removing the module shuts down the
   sound hardware for more power savings.
 
-Mac-on-Linux support
-CONFIG_MOL
-  This option enables low-level support for Mac-on-Linux.
-  MOL lets you run MacOS and Linux simultaneously. Please
-  visit <http://www.maconlinux.org> for more information.
-  If unsure, say Y.
-
 ADB raw keycode support
 CONFIG_MAC_ADBKEYCODES
   This provides support for sending raw ADB keycodes to console
@@ -17148,16 +17449,6 @@
   and iBook computers. 
 
   This driver is also available as a module called gmac.o ( = code
-  which can be inserted in and removed from the running kernel
-  whenever you want). If you want to compile it as a module, say M
-  here and read Documentation/modules.txt.
-
-Symbios 53c885 (Synergy ethernet) support
-CONFIG_NCR885E
-  This is and Ethernet driver for the dual-function NCR 53C885
-  SCSI/Ethernet controller.
-
-  This driver is also available as a module called ncr885e.o ( = code
   which can be inserted in and removed from the running kernel
   whenever you want). If you want to compile it as a module, say M
   here and read Documentation/modules.txt.
