--- Configure.help-2.4.34	2007-07-29 20:39:15.000000000 +0900
+++ Configure.help-2.4.35	2007-07-29 21:03:33.000000000 +0900
@@ -12142,0 +12143,31 @@
+Marvell Yukon Gigabit Ethernet Adapter family support
+CONFIG_SKGE
+  This is an alternate driver for the Marvell Yukon Gigabit Ethernet
+  family. It is a backport of version 1.6 for kernel 2.6. The vendor's
+  one is normally recommended (sk98lin), but under some circumstances, it
+  is known to have trouble (eg: sending UDP only on old chips). This driver
+  is not very fast an may lead to higher CPU loads than the original one
+  since it does not support NAPI yet, but at least it is reported to work
+  and is maintained in 2.6. Linking it with the kernel is not recommended
+  since it may conflict with sk98lin.
+
+  If you want to compile this driver as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want),
+  say M here and read Documentation/modules.txt. This is recommended.
+  The module will be called skge.o.
+
+Marvell Yukon 2 Gigabit Ethernet Adapter family support
+CONFIG_SKY2
+  This is an alternate driver for the Marvell Yukon 2 Gigabit Ethernet
+  family. It is a backport of version 1.5 for kernel 2.6. The vendor's
+  one is normally recommended (sk98lin), but under some circumstances, it
+  is known to have trouble (eg: sending UDP only on old chips). This driver
+  is not very fast an may lead to higher CPU loads than the original one
+  since it does not support NAPI yet, but at least it is reported to work
+  and is maintained in 2.6. Linking it with the kernel is not recommended
+  since it may conflict with sk98lin.
+
+  If you want to compile this driver as a module ( = code which can be
+  inserted in and removed from the running kernel whenever you want),
+  say M here and read Documentation/modules.txt. This is recommended.
+  The module will be called sky2.o.
@@ -20499,0 +20531,7 @@
+W83627HF/F/HG/G Watchdog
+CONFIG_WDT_W83627
+  This is a driver for the hardware watchdog on the W83627HF chipset.
+  To compile this driver as a module say M here. The module will be
+  named wdt83627.o
+  Most people will say N.
+
