Main Page Class Hierarchy Data Structures File List Data Fields Globals

# PV2Way324ConnectOptions Class Reference

`#include <pv_2way_h324m_types.h>`

Inheritance diagram for PV2Way324ConnectOptions:

## Public Methods
| PV2Way324ConnectOptions (uint32 aDisconnectTimeoutInterval)
| PV2Way324ConnectOptions ()
virtual | ~PV2Way324ConnectOptions ()
virtual void | GetConnectInfoClassName (OSCL_wString &aClassName)
## Data Fields
uint32 | iDisconnectTimeoutInterval

## Detailed Description

PV2Way324ConnectOptions Class

PV2Way324ConnectOptions implements the PV2WayConnectOptions interface and is used for 324M specific initialization.

## Constructor & Destructor Documentation

PV2Way324ConnectOptions::PV2Way324ConnectOptions | ( | uint32 | aDisconnectTimeoutInterval | ) | `[inline]`

  | Constructor Parameters:
  disconnectTimeout | The interval to wait after initiating a disconnect before stopping signalling

PV2Way324ConnectOptions::PV2Way324ConnectOptions | ( |  | ) | `[inline]`

virtual PV2Way324ConnectOptions::~PV2Way324ConnectOptions | ( |  | ) | `[inline, virtual]`

## Member Function Documentation

virtual void PV2Way324ConnectOptions::GetConnectInfoClassName | ( | OSCL_wString & | aClassName | ) | `[inline, virtual]`

  | Retrieves the class name Parameters:
  aClassName | A reference to an OSCL_wString, which is to hold the subclass name, this class will assign the string "CPV2Way324ConnectInfo"
Returns: void Implements PV2WayConnectOptions.

## Field Documentation

uint32 PV2Way324ConnectOptions::iDisconnectTimeoutInterval

| The disconnect timeout interval in units of 100ms

The documentation for this class was generated from the following file:

- pv_2way_h324m_types.h