#/etc/ppp/gprs-connect-chat
# chat script for China Mobile, used HuaWei GTM900-B GPRS module.
TIMEOUT         15
ABORT           "DELAYED"
ABORT           "BUSY"
ABORT           "ERROR"
ABORT           "NO DIALTONE"
ABORT           "NO CARRIER"
TIMEOUT         40
''              \rAT
OK              ATZ
OK              "ATQ0 V1 E1 +FCLASS=0"
OK              AT+CGDCONT=1,"IP","emome"
OK              ATDT*99#
CONNECT         ''
