# mrcImageRefCreate

## Usage

    Usage: mrcImageRefCreate
    Options:
        [-i[nput]            In                  (NULL      ).as(inFile              ) ] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      ).as(outFile             ) ] :Essential :OutputDataFile
        [-p[osition]         iP                  (0         ).as(Real                )
                             iW                  (0         ).as(Real                )
                             iA                  (0         ).as(Real                ) ] :Optional  :Position of Center of model creation. Phi(degree) ,Omega(degree) ,Alpha(degree)
    :Omega and Alpha range must be around 0 or 180.
        [-w[idth]            Wp                  (360       ).as(Real                )
                             Ww                  (10        ).as(Real                )
                             Wa                  (10        ).as(Real                ) ] :Optional  :Width of Phi(degree,plus minus) ,Omega(degree,plus minus) ,Alpha(degree,plus minus)
        [-d[elta]            Dp                  (5         ).as(Real                )
                             Dw                  (5         ).as(Real                )
                             Da                  (5         ).as(Real                ) ] :Optional  :Interval of model creation(degree) Phi(around Z axis),Omega(Y axis),Alpha(X axis)
        [-x                  Wx                  (NULL      ).as(Integer             ) ] :Optional  :Data length of x in the outputfile.Default:Data length of x in the inputfile
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         ).as(Integer             ) ] :Optional  :Mode