# tiff2mrc

## Usage

    Usage: tiff2mrc
    Options:
        [-i[nput]            inFile              (NULL      ).as(inFile              ) ] :Essential :InputDataFile
        [-o[utput]           outFile             (NULL      ).as(outFile             ) ] :Essential :OutputDataFile
        [-r[esolution]       Resolution          (1.0       ).as(Real                ) ] :Optional  :Resolution[A]
        [-t[ime]             time                (1.0       ).as(Real                ) ] :Optional  :x OptimalTime
        [-d[irnum]           dirnum              (0         ).as(Integer             ) ] :Optional  :tiffDirectoryNumber
        [-I[nverse]                                                                    ] :Optional  :Black<->White
        [-Signed                                                                       ] :Optional  :Original image is Signed or Not: Default unsigned
        [-Offset             Offset              (0.0       ).as(Real                ) ] :Optional  :OffsetValue
        [-Max                Max                 (16        ).as(Real                ) ] :Optional  :MaxValue:2^Max
        [-Min                Min                 (1         ).as(Real                ) ] :Optional  :MinValue:2^Min: without 0
        [-realMin            realMin             (0.0       ).as(Real                ) ] :Optional  :Real MinValue
        [-realMax            realMax             (0.0       ).as(Real                ) ] :Optional  :Real MaxValue
        [-realMaxBit         realMaxBit          (14        ).as(Real                ) ] :Optional  :Real MaxValue Bit
        [-sin                sinFile             (NULL      ).as(inFile              ) ] :Optional  :sin file from Zeiss
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-S[hrink]           Shrink              (8         ).as(Integer             ) ] :Optional  :ShrinkMode
        [-M[ode]             Mode                (0         ).as(Integer             ) ] :Optional  :Mode: mrcMode: Def: if -m 0, -M 0. if -m 1 -M 2
        [-m[ode]             mode                (0         ).as(Integer             ) ] :Optional  :Mode: 0 (Direct), 1(Log10(65535/data))
    ---- mode ----
    0x0000000f bits: Direct or Log
    0x000000f0 bits: Which Color
                     R: 00
                     G: 10
                     B: 20