--- Configure.help-2.4.32	2006-08-14 18:49:35.000000000 +0900
+++ Configure.help-2.4.33	2006-08-14 18:49:56.000000000 +0900
@@ -8151 +8151 @@
-  CONFIG_AIC7XXX_DEBUG_ENBLE option is enabled.  The bits in this mask
+  CONFIG_AIC7XXX_DEBUG_ENABLE option is enabled.  The bits in this mask
@@ -8325 +8325 @@
-  CONFIG_AIC79XX_DEBUG_ENBLE option is enabled.  The bits in this mask
+  CONFIG_AIC79XX_DEBUG_ENABLE option is enabled.  The bits in this mask
@@ -15242,0 +15243,18 @@
+Dummy keyboard driver
+CONFIG_DUMMY_KEYB
+  What is this for?
+
+  Not all systems have keyboards.  Some don't even have a keyboard
+  port.  However, some of those systems have video support and can
+  use the virtual terminal support for display.  However, the virtual
+  terminal code expects a keyboard of some kind.  This driver keeps
+  the virtual terminal code happy by providing it a "keyboard", albeit
+  a very quiet one.
+
+  If you want to use the virtual terminal support but your system
+  does not support a keyboard, define CONFIG_DUMMY_KEYB along with
+  CONFIG_VT.
+
+  This can also be selected lonesome without any VT support (i.e. no
+  monitor or keyboard attached) - just define CONFIG_DUMMY_KEYB.
+
